**REQUIREMENTS NOT MET**

<insert any requirements not met, if applicable (if not applicable, write “N/A”)>

**PROBLEMS ENCOUNTERED**

<insert a brief summary of *all* problems encountered>

**FUTURE WORK/APPLICATIONS**

<insert a brief paragraph describing how the topics covered in this lab could potentially be used for other applications>

THE ABOVE SHOULD BE LIMITED TO THE FIRST PAGE, AND NOTHING ELSE SHOULD BE INCLUDED, WHICH ALSO IMPLIES THAT THIS SENTENCE OF TEXT SHOULD BE REMOVED.

**PRE-LAB EXERCISES**

**i. Which configuration register allows the utilization of an I/O port pin configured as an input? Which configuration registers allow the utilization of an I/O port pin configured as an output?**

**The “in” register of a port allows you to read the port as input.  
 The “out” register of a port allows you to output vales at certain pins.  
 The “outset” register writes a “high” signal to whichever bits are set to “1”  
 The “outclr” register writes a “low” signal to whichever bits are set to "1”  
 The “outtgl” register toggles a signal to whichever bits are set to "1”**

**ii. What is the purpose of the SET/CLR/TGL variants of the DIR and OUT registers?**

**The purpose is to allow you to adjust the signal levels of individual pins without   
Affecting other pins**

**iii. Are the LEDs on the OOTB Switch & LED Backpack active-high, or active-low? Draw a schematic diagram for a single LED circuit with the same activation level used on the backpack, as well as one with the opposite activation level. Also, draw a schematic diagram for a single-pole, single-throw (SPST) switch circuit, using the same pull-up or pull-down resistor condition utilized on the backpack, as well as another switch circuit using the opposite configuration.**

**Led’s are active-low.  
A picture containing sketch, drawing, line art, diagram

Description automatically generated**

**iv. Which I/O ports are utilized for the DIP switches and LEDs on the OOTB Switch & LED Backpack?**

**The led circuits utilize port C  
 The switch circuit utilizes port A**


**v. Would it be possible to interface the OOTB µPAD with an external input device consisting of 24 inputs? If so, describe how many I/O ports would be necessary. If not, explain why.**

**The OOTB has 3 ports with 8 pins each. All ports are configurable as inputs. Therefore, it should  
be possible to connect a 24-pin input device.**

**vi. Assuming a system clock frequency of 2 MHz, a prescaler value of 8, and a desired period of 72 ms, calculate a theoretically-corresponding timer/counter period value two separate times: once using a form of dimensional analysis, providing explanation(s) when appropriate, and another time using the general formula provided within The Most Common Use Case for Timer/Counters.  
A picture containing text, handwriting, font, calligraphy

Description automatically generated**

**vii. Assuming a system clock frequency of 2 MHz, is a period of two seconds achievable when using a 16-bit timer/counter prescaler value of one? If not, determine if there exists any prescaler value that allows for this period under the assumed circumstances, and if there does, list such a value.**

****

**viii. What is the maximum time value (to the nearest millisecond) representable by a timer/counter, if the relevant system clock frequency is 2 MHz? What about for a system clock frequency of 32.768 kHz?**

A picture containing text, handwriting, font, calligraphy

Description automatically generated  
**ix. Create an assembly program to perform the same procedure as in § 3.2 but utilize a prescaler value of two. Perform everything else described in the section for this new context, i.e., experimentally determine which whole-number digital period value provides a corresponding period with the least amount of error, provide an appropriate screenshot of the relevant waveform with the minimal amount of error, including its precise frequency, and provide within the caption of the relevant screenshot the whole-number value that resulted in a minimal amount of error. Finally, describe and explain why there may be any differences between the two contexts, i.e., between using a prescaler value of sixteen, the value in exercise vi, and a prescaler value of two.**

**The program is in section 3, labeled “prelab question number IX”**

**x. Create an assembly program to keep track of elapsing minutes with a timer/counter, i.e., design a “watch” that only has a “minute-hand”. (Hint: Instead of attempting to configure the period of the timer/counter to directly correspond to sixty seconds, configure the period to correspond to one second, and then keep track of how many times this timer/counter overflows [or underflows, if you wish to configure the timer/counter to count down].)**

**The program is in section 3, labeled “prelab question number X”**

**PSEUDOCODE/FLOWCHARTS**

**SECTION 1**

A diagram of a flowchart

Description automatically generated with low confidence **Figure 1:Flowchart for “lab2\_1.asm”. This copies  
the switch circuit register values to the   
output registers for the LED’s**

**SECTION 2**

**A diagram of a flowchart

Description automatically generated with low confidence  
Figure 2: Flowchart for “lab2\_2.asm” with “delay\_10ms” being the only subroutine.  
This toggles pin 0 of port C every 10ms, giving us a 10ms PWM signal.**

**A diagram of a flowchart

Description automatically generated with low confidence  
Figure 3: Flowchart for “delay\_10ms” subroutine.  
“FAUS” creates a delay of 250us by executing 500 single cycle instructions.  
 “ONEKUS” creates a 1000us delay by running “FAUS” 4 times.  
“TENMS” creates a 10000us delay by running “ONEKUS” 10 times.  
Giving us a delay of 10ms.**

**A picture containing text, diagram, screenshot, line

Description automatically generated  
Figure 4: Flowchart for “delay\_X\_10ms”.  
R21 is the multiple of 10ms delays.**

**SECTION 3**

**A diagram of a flowchart

Description automatically generated with low confidence**

**Figure 5: flowchart for “lab2\_3.asm.  
This triggers an output signal every 40ms   
by checking the overflow flag on timer/counter number 0**

**A picture containing text, diagram, plan, technical drawing

Description automatically generated**

**Figure 6: flowchart for “lab2\_prelabquestionx.asm.  
This counts how many minutes have elapsed  
since program began execution.**

**PROGRAM CODE**

**SECTION 1**

;Lab 2, Section 1

;Name: Steven Miller

;Class #: 11318

;PI Name: Anthony Stross

;Description: Allows control of LED's through switch circuit

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*INCLUDES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.include "ATxmega128a1udef.inc"

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF INCLUDES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*EQUATES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.EQU INPUT = 0B00000000

.EQU OUTPUT = 0B11111111

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF EQUATES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*DEFS\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF DEFS\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*MEMORY CONFIGURATION\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*END OF MEMORY CONFIGURATION\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*MAIN PROGRAM\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.CSEG

.org 0x0100

MAIN:

;set port directions

LDI R16, INPUT

STS PORTA\_DIR , R16

LDI R16, OUTPUT

STS PORTC\_DIR , R16

;loop for actual led and switch circuits

LOOP:

;copy load value from switch registers into led registers

LDS R16, PORTA\_IN

STS PORTC\_OUT,R16

RJMP LOOP

;\*\*\*\*\*\*\*\*\*\*\*END MAIN PROGRAM\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

**Section 2  
Original code to create software delay of 10ms**

;Lab 2, Section 2

;Name: Steven Miller

;Class #: 11318

;PI Name: Anthony Stross

;Description: Implements software delays

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*INCLUDES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.include "ATxmega128a1udef.inc"

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF INCLUDES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*EQUATES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.EQU sramend = 0x3fff ;top of stack

.EQU srambegin = 0x2000 ;bottom of stack

.EQU input = 0b00000000

.EQU output = 0b11111111

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF EQUATES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*DEFS\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.DEF ms\_r16 = r16

.DEF us\_r17 = r17

.DEF zero\_r18 = r18

.DEF one\_r19 = r19

.DEF four\_r20 = r20

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF DEFS\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*MAIN PROGRAM\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.CSEG

.org 0x0100

MAIN:

;initialize stack pointer

ldi r16, low(sramend)

out CPU\_SPL, r16

ldi r16, high(sramend)

out CPU\_SPH, r16

;set port directions

LDI R22, output

STS PORTC\_DIR , R22

;initialize registers

ldi zero\_r18,0

ldi one\_r19,1

ldi four\_r20,4

;loop to call subroutine

LOOP:

rcall delay\_10ms

STS PORTC\_OUTTGL,R22

RJMP LOOP

;\*\*\*\*\*\*\*\*\*\*\*END MAIN PROGRAM\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*SUBROUTINES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

; Subroutine Name: delay\_10ms

; performs a series of instructions for 10ms

; Inputs: none

; Ouputs: none

; Affected: r16, r17,r19,r20

delay\_10ms:

ldi ms\_r16,0

ldi us\_r17,0

tenms:

ldi four\_r20, 0

;1ms

onekus:

ldi us\_r17,0

;250us

faus:

add us\_r17,one\_r19

cpi us\_r17,250

brne faus

add four\_r20,one\_r19

cpi four\_r20,4

;branch if 1ms

brne onekus

add ms\_r16,one\_r19

;branch if 10 ms

cpi ms\_r16,10

brne tenms

ret

**Code after adjustment for imprecision**

;Lab 2, Section 2

;Name: Steven Miller

;Class #: 11318

;PI Name: Anthony Stross

;Description: Implements software delays

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*INCLUDES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.include "ATxmega128a1udef.inc"

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF INCLUDES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*EQUATES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.EQU sramend = 0x3fff ;top of stack

.EQU srambegin = 0x2000 ;bottom of stack

.EQU input = 0b00000000

.EQU output = 0b11111111

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF EQUATES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*DEFS\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.DEF ms\_r16 = r16

.DEF us\_r17 = r17

.DEF zero\_r18 = r18

.DEF one\_r19 = r19

.DEF four\_r20 = r20

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF DEFS\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*MAIN PROGRAM\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.CSEG

.org 0x0100

MAIN:

;initialize stack pointer

ldi r16, low(sramend)

out CPU\_SPL, r16

ldi r16, high(sramend)

out CPU\_SPH, r16

;set port directions

LDI R22, output

STS PORTC\_DIR , R22

;initialize registers

ldi zero\_r18,0

ldi one\_r19,1

ldi four\_r20,4

;loop to call subroutine

LOOP:

rcall delay\_10ms

STS PORTC\_OUTTGL,R22

RJMP LOOP

;\*\*\*\*\*\*\*\*\*\*\*END MAIN PROGRAM\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*SUBROUTINES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

; Subroutine Name: delay\_10ms

; performs a series of instructions for 10ms

; Inputs: none

; Ouputs: none

; Affected: r16, r17,r19,r20

delay\_10ms:

ldi ms\_r16,0

ldi us\_r17,0

tenms:

ldi four\_r20, 0

;1ms

onekus:

ldi us\_r17,0

;250us

faus:

add us\_r17,one\_r19

cpi us\_r17,253

brne faus

add four\_r20,one\_r19

cpi four\_r20,2

;branch if 1ms

brne onekus

add ms\_r16,one\_r19

;branch if 10 ms

cpi ms\_r16,10

brne tenms

ret

**Including “delay\_x\_10ms” subroutine. Delays for .04s.**

;Lab 2, Section 2

;Name: Steven Miller

;Class #: 11318

;PI Name: Anthony Stross

;Description: Implements software delays

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*INCLUDES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.include "ATxmega128a1udef.inc"

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF INCLUDES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*EQUATES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.EQU sramend = 0x3fff ;top of stack

.EQU srambegin = 0x2000 ;bottom of stack

.EQU input = 0b00000000

.EQU output = 0b11111111

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF EQUATES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*DEFS\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.DEF ms\_r16 = r16

.DEF us\_r17 = r17

.DEF zero\_r18 = r18

.DEF one\_r19 = r19

.DEF four\_r20 = r20

.DEF multiple\_r21 = r21

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF DEFS\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*MAIN PROGRAM\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.CSEG

.org 0x0100

MAIN:

;initialize stack pointer

ldi r16, low(sramend)

out CPU\_SPL, r16

ldi r16, high(sramend)

out CPU\_SPH, r16

;set port directions

LDI R22, output

STS PORTC\_DIR , R22

;initialize registers

ldi zero\_r18,0

ldi one\_r19,1

ldi four\_r20,4

;loop to call subroutine

LOOP:

ldi multiple\_r21,1

rcall delay\_x\_10ms

STS PORTC\_OUTTGL,R22  
RJMP LOOP

;\*\*\*\*\*\*\*\*\*\*\*END MAIN PROGRAM\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*SUBROUTINES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

; Subroutine Name: delay\_10ms

; performs a series of instructions for 10ms

; Inputs: none

; Ouputs: none

; Affected: r16, r17,r19,r20

delay\_10ms:

ldi ms\_r16,0

ldi us\_r17,0

tenms:

ldi four\_r20, 0

;1ms

onekus:

ldi us\_r17,0

;250us

faus:

add us\_r17,one\_r19

cpi us\_r17,253

brne faus

add four\_r20,one\_r19

cpi four\_r20,2

;branch if 1ms

brne onekus

add ms\_r16,one\_r19

;branch if 10 ms

cpi ms\_r16,10

brne tenms

ret

; Subroutine Name: delay\_x\_10ms

; delays a select multiple of 10ms

; Inputs: r21

; Ouputs: none

; Affected: r16,r17,r19,r20,r21

delay\_x\_10ms:

push r21

loopx:

cpi multiple\_r21,0

breq exit

call delay\_10ms

dec multiple\_r21

rjmp loopx

exit:

pop r21

ret

**Section 3**

;Lab 2, Section 3

;Name: Steven Miller

;Class #: 11318

;PI Name: Anthony Stross

;Description: Implements software delay using timer

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*INCLUDES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.include "ATxmega128a1udef.inc"

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF INCLUDES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*EQUATES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.EQU input = 0b00000000

.EQU output = 0b11111111

;.EQU div2 = 0b00000010

.EQU prescalar = 8

.EQU sysclk = 2000000

.EQU desiredperiod = .04 ;40ms

.EQU reciprocol = 1/.04 ;idk how to spell reciprocol

.EQU offset = 175 ;correcting for imprecision

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF EQUATES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*DEFS\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF DEFS\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*MAIN PROGRAM\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.CSEG

.org 0x0100

MAIN:

;initialize port c for output

ldi r16, output

sts PORTC\_DIR, r16

;initialize count register

ldi r16,0

sts TCC0\_CNT, r16

sts TCC0\_CNT+1,r16

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*NOTES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;if we want to achieve a period of 40 ms with a prescalar of 8

;and a frequency of 2mhz, that equates to:

;ticks = (2000000cycles/second)/(8cycles/tick)\*.04seconds = 10000 ticks

;ticks = (systemclock/prescalar) / (1/desiredperiod)

;it also may be a good idea to add a number that corrects

;for any imprecision

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF NOTES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;initialize period register

ldi r16,low(((sysclk/prescalar)/reciprocol)+offset)

sts TCC0\_PER, r16

ldi r16,high(((sysclk/prescalar)/reciprocol)+offset)

sts TCC0\_PER+1,r16

;initialize clksel

ldi r16, CLK\_PSADIV\_8\_gc

sts TCC0\_CTRLA,r16

;toggle output port

loop:

lds r17,TCC0\_INTFLAGS

;check ov flag

andi r17,0b00000001

cpi r17,1

;branch if we have overflow

breq toggleoutput

;else

rjmp loop

;if we have an overflow

toggleoutput:

;toggle outputs

ldi r17,output

sts PORTC\_OUTTGL, r17

;clear ov flag

ldi r17, 0b00000001

sts TCC0\_INTFLAGS,r17

rjmp loop

end:

rjmp end

;\*\*\*\*\*\*\*\*\*\*\*END MAIN PROGRAM\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

**Section 3, prelab question 9**;Lab 2, prelab question ix

;Name: Steven Miller

;Class #: 11318

;PI Name: Anthony Stross

;Description: Implements software delay using timer with prescalar

;value of 2

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*INCLUDES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.include "ATxmega128a1udef.inc"

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF INCLUDES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*EQUATES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.EQU input = 0b00000000

.EQU output = 0b11111111

;.EQU div2 = 0b00000010

.EQU prescalar = 2

.EQU sysclk = 2000000

.EQU desiredperiod = .04 ;40ms

.EQU reciprocol = 1/.04 ;idk how to spell reciprocol

.EQU offset = 255 ;correcting for imprecision

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF EQUATES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*DEFS\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF DEFS\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*MAIN PROGRAM\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.CSEG

.org 0x0100

MAIN:

;initialize port c for output

ldi r16, output

sts PORTC\_DIR, r16

;initialize count register

ldi r16,0

sts TCC0\_CNT, r16

sts TCC0\_CNT+1,r16

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*NOTES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;if we want to achieve a period of 40 ms with a prescalar of 2

;and a frequency of 2mhz, that equates to:

;ticks = (2000000cycles/second)/(2cycles/tick)\*.04seconds = 40000 ticks

;ticks = (systemclock/prescalar) / (1/desiredperiod)

;it also may be a good idea to add a number that corrects

;for any imprecision

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF NOTES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;initialize period register

ldi r16,low(((sysclk/prescalar)/reciprocol)+offset)

sts TCC0\_PER, r16

ldi r16,high(((sysclk/prescalar)/reciprocol)+offset)

sts TCC0\_PER+1,r16

;initialize clksel

ldi r16, CLK\_PSADIV\_2\_gc

sts TCC0\_CTRLA,r16

;toggle output port

loop:

lds r17,TCC0\_INTFLAGS

;check ov flag

andi r17,0b00000001

cpi r17,1

;branch if we have overflow

breq toggleoutput

;else

rjmp loop

;if we have an overflow

toggleoutput:

;toggle outputs

ldi r17,output

sts PORTC\_OUTTGL, r17

;clear ov flag

ldi r17, 0b00000001

sts TCC0\_INTFLAGS,r17

rjmp loop

end:

rjmp end

;\*\*\*\*\*\*\*\*\*\*\*END MAIN PROGRAM\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

**A screenshot of the waveform is located in the appendix in figure insert figure number here**

**When the prescalar value is set to 2,**

**Section 3, prelab question 10**

;Lab 2, prelab question x

;Name: Steven Miller

;Class #: 11318

;PI Name: Anthony Stross

;Description: counts how many minutes have elapsed since start of program

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*INCLUDES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.include "ATxmega128a1udef.inc"

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF INCLUDES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*EQUATES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.EQU prescalar = 64

.EQU sysclk = 2000000

.EQU desiredperiod = 1 ;1000ms

.EQU reciprocol = 1/1 ;idk how to spell reciprocol

.EQU offset = 590 ;correcting for imprecision

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF EQUATES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*DEFS\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.DEF second\_r18 = r18

.DEF minute\_r19 = r19

.DEF one\_r20 = r20

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF DEFS\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;\*\*\*\*\*\*\*\*\*\*\*MAIN PROGRAM\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

.CSEG

.org 0x0100

MAIN:

;initialize registers

ldi second\_r18,60

ldi minute\_r19,0

ldi one\_r20,1

;initialize count register

ldi r16,0

sts TCC0\_CNT, r16

sts TCC0\_CNT+1,r16

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*NOTES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;if we want to achieve a period of 40 ms with a prescalar of 8

;and a frequency of 2mhz, that equates to:

;ticks = (2000000cycles/second)/(64cycles/tick)\*1seconds = 31250 ticks

;ticks = (systemclock/prescalar) / (1/desiredperiod)

;it also may be a good idea to add a number that corrects

;for any imprecision

;\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*END OF NOTES\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

;initialize period register

ldi r16,low(((sysclk/prescalar)/reciprocol)+offset)

sts TCC0\_PER, r16

ldi r16,high(((sysclk/prescalar)/reciprocol)+offset)

sts TCC0\_PER+1,r16

;initialize clksel

ldi r16, TC\_CLKSEL\_DIV64\_gc

sts TCC0\_CTRLA,r16

loop:

lds r17,TCC0\_INTFLAGS

;check ov flag

andi r17,0b00000001

cpi r17,1

;branch if we have overflow

breq decrementsecond

;else

rjmp loop

decrementsecond:

;decrement "second" register

dec second\_r18

;clear ov flag

ldi r17, 0b00000001

sts TCC0\_INTFLAGS,r17

;see if we hit a minute

cpi second\_r18, 0

brne loop

add minute\_r19,one\_r20

rjmp loop

end:

rjmp end

;\*\*\*\*\*\*\*\*\*\*\*END MAIN PROGRAM\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

**APPENDIX**

**A screen shot of a graph

Description automatically generated with medium confidence  
Figure x: Software Delay without adjustment. The red underlined is the length of the delay.**

**A screen shot of a graph

Description automatically generated with low confidence  
Figure X: Software Delay after reducing number of times “ONEKUS” runs “FAUS” from 4 to 2**

**A screen shot of a graph

Description automatically generated with medium confidence  
Figure X: Software Delay after reducing number of times “ONEKUS” runs “FAUS” from 4 to 2, while also increasing number of times “FAUS” iterates from 250 to 253.**

**A screen shot of a graph

Description automatically generated with low confidence  
Figure X: .04 second delay using software delay**

**A screen shot of a graph

Description automatically generated with low confidence  
Figure x: .04 second delay using timer/counter number 0.  
An offset of 175 had to be added to account for imprecision.**

**A screen shot of a graph

Description automatically generated with medium confidence  
 Figure X: .04 delay when prescalar value is set to 2.  
The offset is set to 760.**